
Specification

Extrusion: FLAT 30



1. The extrusion shall be made of aluminum alloy EN AW 6060 T66.
2. The extrusion shall be available in following surface finishes:
   * Blank
   * Anodized natural (thickness 15µm)
   * Anodized black (thickness 15µm)
   * Coated with polyester powder-coating in all standard RAL-colors
3. The extrusion shall serve as cooling for the LEDs.
4. The extrusion shall have following dimensions 30m x 5mm.
5. The extrusion shall be available in lengths up to 6m.
6. The extrusion shall fit a PCB of maximum 13mm
7. The extrusion shall weigh max 0,25 kg/m