Specification

Extrusion: RECTANG 22



1. The extrusion shall be made of aluminum alloy EN AW 6060.
2. The extrusion shall be available in following surface finishes:
	* Blank
	* Anodized natural (thickness 15µm)
	* Anodized black (thickness 15µm)
	* Coated with polyester powder-coating in all standard RAL-colors
3. The extrusion shall serve as cooling for the LEDs.
4. The extrusion shall have following dimensions 22m x 13mm.
5. The extrusion shall be available in lengths up to 6m.
6. The extrusion shall fit a PCB of maximum 17mm.